SECTION 01 58 00 PROJECT IDENTIFICATION

1. GENERAL
   1. TEMPORARY PROJECT SIGNAGE
      1. Contractor shall install and maintain a project informational sign(s) provided by the University at a location(s) designated by the University’s Representative.

|  |
| --- |
| The following paragraph is for projects in existing buildings. |

* + 1. At every door and barricade separating the project work and staging areas from areas not included in the project work area, the Contractor shall provide, install and continuously maintain a construction warning sign. The 11 inch by 17 inch construction warning sign shall be reproduced from camera-ready text provided by the University’s Representative, shall be plastic laminated on heavy cardstock and shall be securely affixed at eye level to the door or barricade.

|  |
| --- |
| The following paragraphs are for major new projects only. Delete paragraphs that are not applicable. |

* + 1. No signs or advertisements will be permitted on the Project site, including company names and logos on job site trailers, except with express permission of University's Representative.
    2. Provide one 4 feet by 8 feet Project sign to be located at the Project site mounted on two 6 by 6 inch posts set in concrete in the location identified by the University Representative.
    3. Format, colors and content for production of the sign shall be provided by the University’s Representative.
    4. Contractor must coordinate the fabrication and installation. The sign may be produced by the University’s Sign Shop (for a fee), or a third party sign fabricator.

1. PRODUCTS (NOT USED)
2. EXECUTION (NOT USED)

END OF SECTION 01 58 00